|  | 10.3 | IP Addresses within the IP Header
| 10.3.3 | IP header source and destination fields

The IP address contains the information that is necessary to route a packet through the network. Each source and destination address field contains a 32 bit address. The source address field contains the IP address of the device that sends the packet. The destination field contains the IP address of the device that receives the packet.

| Web Links
| IP Addressing Architecture