Cabling installation requirements :: | 18/55

| Requirements

- Cable and components shall be visually inspected for proper installation.

Recommendations

- Cable stress, such as that caused by tension in suspended cable runs and tightly cinched bundles, should be minimized.
- Cable ties used to bundle cables should be applied loosely to allow the cable tie to slide around the cable bundle.
- The cable ties should not be cinched so tightly as to deform the cable sheath. Cable placement should not deform the cable sheath.

Cabling installation requirements :: | 18/55