Patch cords, equipment cords, work area cords, and jumpers :: | 21/55

| Requirements

- To minimize return loss degradation, unjacketed jumper wire shall not be made in the field by removing the jacket in large part or it's entirety from a previously jacketed cable.

Recommendations

- Cross-connect jumpers and cables used for patch cords should be of the same performance category or higher as the horizontal cables to which they connect. Patch cords are also used for equipment cords and work area cords.
- Patch cords should not be field terminated.

Patch cords, equipment cords, work area cords, and jumpers :: | 21/55