failure domain

  Area in which a failure has occurred in a Token Ring, defined by the information contained in a beacon. When a station detects a serious problem with the network (such as a cable break), it sends a beacon frame that includes the station reporting the failure, its NAUN, and everything in between. Beaconing in turn initiates a process called autoreconfiguration. See also autoreconfiguration, beacon, and NAUN.

fan-out unit

  Device that allows multiple devices on a network to communicate using a single network attachment.

fantail

  Panel of I/O connectors that attaches to an equipment rack, providing easy access for data connections to a LightStream 2020 ATM switch. See also applique.

Fast Ethernet

  Any of a number of 100-Mbps Ethernet specifications. Fast Ethernet offers a speed increase ten times that of the 10BASE-T Ethernet specification, while preserving such qualities as frame format, MAC mechanisms, and MTU. Such similarities allow the use of existing 10BASE-T applications and network management tools on Fast Ethernet networks. Based on an extension to the IEEE 802.3 specification. Compare with Ethernet. See also 100BASE-FX, 100BASE-T, 100BASE-T4, 100BASE-TX, 100BASE-X, and IEEE 802.3.

Fast Ethernet Interface Processor

  See FEIP.

Fast Sequenced Transport

  See FST.

Fast Serial Interface Processor

  See FSIP.

fast switching

  Cisco feature whereby a route cache is used to expedite packet switching through a router. Contrast with slow switching.

fault management

  One of five categories of network management defined by ISO for management of OSI networks. Fault management attempts to ensure that network faults are detected and controlled. See also accounting management, configuration management, performance management, and security management.

FCC

  Federal Communications Commission. U.S. government agency that supervises, licenses, and controls electronic and electromagnetic transmission standards.

fcload

  Function card load. Low-level software module in the LightStream 2020 ATM switch that is invoked by higher-level modules to load software from the NP to a function card.

FCS

  Frame check sequence. Refers to the extra characters added to a frame for error control purposes. Used in HDLC, Frame Relay, and other data link layer protocols.

FDDI

  Fiber Distributed Data Interface. LAN standard, defined by ANSI X3T9.5, specifying a 100-Mbps token-passing network using fiber-optic cable, with transmission distances of up to 2 km. FDDI uses a dual-ring architecture to provide redundancy. Compare with CDDI and FDDI II.

FDDI II

  ANSI standard that enhances FDDI. FDDI II provides isochronous transmission for connectionless data circuits and connection-oriented voice and video circuits. Compare with FDDI.

FDDI Interface Processor

  See FIP.

FDM

  Frequency-division multiplexing. Technique whereby information from multiple channels can be allocated bandwidth on a single wire based on frequency. Compare with ATDM, statistical multiplexing, and TDM.

FECN

  Forward explicit congestion notification. Bit set by a Frame Relay network to inform DTE receiving the frame that congestion was experienced in the path from source to destination. DTE receiving frames with the FECN bit set can request that higher-level protocols take flow-control action as appropriate. Compare with BECN.

Federal Communications Commission

  See FCC.

Federal Networking Council

  See FNC.

FEIP

  Fast Ethernet Interface Processor. Interface processor on the Cisco 7000 series routers. The FEIP supports up to two 100-Mbps 100BASE-T ports.

FEP

  Front-end processor. Device or board that provides network interface capabilities for a networked device. In SNA, typically an IBM 3745 device.

FF

  See frame forwarding.

Fiber Distributed Data Interface

  See FDDI.

fiber-optic cable

  Physical medium capable of conducting modulated light transmission. Compared with other transmission media, fiber-optic cable is more expensive, but is not susceptible to electromagnetic interference, and is capable of higher data rates. Sometimes called optical fiber.

fiber-optic interrepeater link

  See FOIRL.

FID0

  Format indicator 0. One of several formats that an SNA TH can use. An FID0 TH is used for communication between an SNA node and a non-SNA node. See also TH.

FID1

  Format indicator 1. One of several formats that an SNA TH can use. An FID1 TH encapsulates messages between two subarea nodes that do not support virtual and explicit routes. See also TH.

FID2

  Format indicator 2. One of several formats that an SNA TH can use. An FID2 TH is used for transferring messages between a subarea node and a PU 2, using local addresses. See also TH.

FID3

  Format indicator 3. One of several formats that an SNA TH can use. An FID3 TH is used for transferring messages between a subarea node and a PU 1, using local addresses. See also TH.

FID4

  Format indicator 4. One of several formats that an SNA TH can use. An FID4 TH encapsulates messages between two subarea nodes that are capable of supporting virtual and explicit routes. See also TH.

field-replaceable unit

  See FRU.

file transfer

  Popular network application that allows files to be moved from one network device to another.

File Transfer, Access, and Management

  See FTAM.

File Transfer Protocol

  See FTP.

filter

  Generally, a process or device that screens network traffic for certain characteristics, such as source address, destination address, or protocol, and determines whether to forward or discard that traffic based on the established criteria.

FIP

  FDDI Interface Processor. Interface processor on the Cisco 7000 series routers. The FIP supports SASs, DASs, dual homing, and optical bypass, and contains a 16-mips processor for high-speed (100-Mbps) interface rates. The FIP complies with ANSI and ISO FDDI standards.

firewall

  Router or access server, or several routers or access servers, designated as a buffer between any connected public networks and a private network. A firewall router uses access lists and other methods to ensure the security of the private network.

firmware

  Software instructions set permanently or semipermanently in ROM.

fish tape

  Retractable coil of steel tape used to guide cable through a wall from above or below.

flapping

  Routing problem where an advertised route between two nodes alternates (flaps) back and forth between two paths due to a network problem that causes intermittent interface failures.

Flash memory

  Technology developed by Intel and licensed to other semiconductor companies. Flash memory is nonvolatile storage that can be electrically erased and reprogrammed. Allows software images to be stored, booted, and rewritten as necessary.

flash update

  Routing update sent asynchronously in response to a change in the network topology. Compare with routing update.

fldsup account

  One of the four default user accounts that are created in the factory on each LightStream 2020 ATM switch. The fldsup account is for the use of field service personnel. Its default interface is the bash shell. See also bash.

flooding

  Traffic passing technique used by switches and bridges in which traffic received on an interface is sent out all of the interfaces of that device except the interface on which the information was originally received.

flow

  Stream of data traveling between two endpoints across a network (for example, from one LAN station to another). Multiple flows can be transmitted on a single circuit.

flow control

  Technique for ensuring that a transmitting entity, such as a modem, does not overwhelm a receiving entity with data. When the buffers on the receiving device are full, a message is sent to the sending device to suspend the transmission until the data in the buffers has been processed. In IBM networks, this technique is called pacing.

FM

  Frequency modulation. Modulation technique in which signals of different frequencies represent different data values. Compare with AM and PAM. See also modulation.

FNC

  Federal Networking Council. Group responsible for assessing and coordinating U.S. federal agency networking policies and needs.

FOIRL

  Fiber-optic interrepeater link. Fiber-optic signaling methodology based on the IEEE 802.3 fiber-optic specification. FOIRL is a precursor of the 10BASE-FL specification, which is designed to replace it. See also 10BASE-FL.

format indicator 0

  See FID0.

format indicator 1

  See FID1.

format indicator 2

  See FID2.

format indicator 3

  See FID3.

format indicator 4

  See FID4.

forward channel

  Communications path carrying information from the call initiator to the called party.

forward delay interval

  Amount of time an interface spends listening for topology change information after that interface has been activated for bridging and before forwarding actually begins.

forward explicit congestion notification

  See FECN.

forwarding

  Process of sending a frame toward its ultimate destination by way of an internetworking device.

forwarding priority

  See transmit priority.

Fourier transform

  Technique used to evaluate the importance of various frequency cycles in a time series pattern.

four-part dotted notation

  See dot address.

fractional T1

  See channelized T1.

FRAD

  Frame Relay access device. Any network device that provides a connection between a LAN and a Frame Relay WAN. See also Cisco FRAD and FRAS.

fragment

  Piece of a larger packet that has been broken down to smaller units.

fragmentation

  Process of breaking a packet into smaller units when transmitting over a network medium that cannot support the original size of the packet. See also reassembly.

frame

  Logical grouping of information sent as a data link layer unit over a transmission medium. Often refers to the header and trailer, used for synchronization and error control, that surround the user data contained in the unit. The terms datagram, message, packet, and segment are also used to describe logical information groupings at various layers of the OSI reference model and in various technology circles.

frame check sequence

  See FCS.

frame forwarding

  Interface on the LightStream 2020 ATM switch that allows any traffic based on HDLC or SDLC frames to traverse the ATM network. Frame forwarding circuits are port-to-port, and only one PVC is allowed between a pair of ports. Frame forwarding is supported by the low-speed interface module, which offers V.35, EIA/TIA-449, or X.21 physical interfaces. Sometimes abbreviated FF.

Frame Relay

  Industry-standard, switched data link layer protocol that handles multiple virtual circuits using HDLC encapsulation between connected devices. Frame Relay is more efficient than X.25, the protocol for which it is generally considered a replacement. See also X.25.

Frame Relay Access Device

  See FRAD.

Frame Relay Access Support

  See FRAS.

Frame Relay bridging

  Bridging technique, described in RFC 1490, that uses the same spanning-tree algorithm as other bridging functions, but allows packets to be encapsulated for transmission across a Frame Relay network.

frame switch

  See LAN switch.

FRAS

  Frame Relay Access Support. Cisco IOS software feature that allows SDLC, Token Ring, Ethernet, and Frame Relay-attached IBM devices to connect to other IBM devices across a Frame Relay network. See also FRAD.

free-trade zone

  Part of an AppleTalk internetwork that is accessible by two other parts of the internetwork that are unable to directly access one another.

frequency

  Number of cycles, measured in hertz, of an alternating current signal per unit time.

frequency-division multiplexing

  See FDM.

frequency modulation

  See FM.

from switch unit

  See FSU.

front end

  Node or software program that requests services of a back end. See also back end, client, and server.

front-end processor

  See FEP.

FRU

  Field-replaceable unit. Hardware component that can be removed and replaced by Cisco-certified service providers. Typical FRUs include cards, power supplies, and chassis components.

FSIP

  Fast Serial Interface Processor. The default serial interface processor for Cisco 7000 series routers. The FSIP provides four or eight high-speed serial ports.

FST

  Fast Sequenced Transport. Connectionless, sequenced transport protocol that runs on top of the IP protocol. SRB traffic is encapsulated inside of IP datagrams and is passed over an FST connection between two network devices (such as routers). Speeds up data delivery, reduces overhead, and improves the response time of SRB traffic.

FSU

  From switch unit. Subsystem of each line card on a LightStream 2020 ATM switch that accepts calls from the switch card, verifies their checksums, and passes them to the reassembly unit. The FSU selectively drops cells if the network becomes congested.

FTAM

  File Transfer, Access, and Management. In OSI, an application layer protocol developed for network file exchange and management between diverse types of computers.

FTP

  File Transfer Protocol. Application protocol, part of the TCP/IP protocol stack, used for transferring files between network nodes. FTP is defined in RFC 959.

full duplex

  Capability for simultaneous data transmission between a sending station and a receiving station. Compare with half duplex and simplex.

full mesh

  Term describing a network in which devices are organized in a mesh topology, with each network node having either a physical circuit or a virtual circuit connecting it to every other network node. A full mesh provides a great deal of redundancy, but because it can be prohibitively expensive to implement, it is usually reserved for network backbones. See also mesh and partial mesh.

function card

  Line card or an NP card in a LightStream 2020 ATM switch.

function card load

  See fcload.

Fuzzball

  Digital Equipment Corporation LSI-11 computer system running IP gateway software. The NSFnet used these systems as backbone packet switches.