Test parameters :: | 27/55

| The primary field test parameters are:

1. Wire map
2. Length
3. Insertion loss
4. Near-end crosstalk (NEXT)
5. Power sum near-end crosstalk (PSNEXT)
6. Equal-level far-end crosstalk (ELFEXT)
7. Power sum equal-level far-end crosstalk (PSELFEXT)
8. Return loss
9. Propagation delay
10. Delay skew

NOTE - Other parameters such as longitudinal balance and longitudinal impedance, which may be of importance to specific networking applications, are under study.

Test parameters :: | 27/55