|  | 8.4 | Planning Structured Cabling: Selection Practice
| 8.4.8 | Closet G

Room G is relatively small. Its dimensions are approximately 1.8 m wide x .9 m deep. The outside wall for room G is only a partial wall. It does not reach all the way to the 3.7 m high dropped ceiling. It only extends from the floor, and is of drywall construction. The two back walls do extend all the way to the dropped ceiling and are of concrete block construction. One electrical outlet is located along the longer of the two back walls. Room G does not possess its own lighting fixture. Lighting is provided by florescent lighting fixtures in the corridor, and in a shared work space. There is no door into room G, however, the entryway is .9 m wide.

The floor is carpeted. There are no air vents from the heating and cooling duct into room G. The nearest vent is located approximately 4.6 m away. The nearest thermostat is located on the wall opposite the entry into room G. Currently, the space provided by room G houses the water cooler, a small microwave, and a small refrigerator.