Insertion loss :: | 30/55

| Insertion loss is a measure of signal loss in the permanent link or channel.

- Worst case insertion loss relative to the maximum insertion loss allowed shall be reported.

The link insertion loss is the sum of:

1. insertion loss of all connecting hardware
2. insertion loss of 10 m (32.8 ft) of patch and equipment cord total to make connections on each end of the channel configuration (there is no patch or equipment cord length allotment for the permanent link).
3. insertion loss of the cable segment, based on the prorated insertion loss relative to the insertion loss of a 100 m (328 ft) cable segment.

Insertion loss :: | 30/55