|  | 8.4 | Planning Structured Cabling: Selection Practice
| 8.4.7 | Closet F

Room F is centrally located near the front of the building, next to the main entry, and behind the receptionist's desk. Currently it is used as a cloak room. There are two doors into the room. Each door is approximately .9 m wide, and each swings out when opened. Neither door has a lock. Lighting is provided by an incandescent light fixture. There are two light switches that turn the overhead light on and off. They are located just inside each door.

There are no heating or cooling vents into the room. The nearest thermostat is located along the corridor wall outside Room 118. The floor is carpeted. The room has one electrical outlet. It is located along the wall behind the receptionist's desk in the lobby. Also, Room F has high voltage power lines running through its outside walls.