|  | 9.3 | Basics of Cable Installations
| 9.3.3 | TIA/EIA-606 specifications for labeling cable

TIA/EIA-606 specifies that each hardware termination unit have some kind of unique identifier. This identifier must be marked on each termination hardware unit, or on its label. When identifiers are used at the work area, station terminations must have a label on the faceplate, the housing, or the connector itself. All labels, whether they are adhesive or insertable, must meet legibility, defacement, and adhesion requirements as specified in UL969.

| Web Links
| Cabling Glossary
| Cable Termination and Installation