Work area telecommunications outlet/connector :: | 10/55

| 100 Ohm balanced twisted-pair telecommunications outlet/connector Requirements

- Each four-pair cable shall be terminated in an eight-position modular outlet at the work area.
- Telecommunications outlet/connectors for 100 Ohm UTP and ScTP cabling shall meet the requirements of ANSI/TIA/EIA-568-B.2 and the terminal marking and mounting requirements specified in ANSI/TIA/EIA-570-A.
- Pin/pair assignments shall be as shown below. The T568B pin/pair assignments may be used if necessary to accommodate certain 8-pin cabling systems.
- These illustrations depict the front view of the telecommunications outlet/connector.

Work area telecommunications outlet/connector :: | 10/55