|  | 9.2 | RJ-45 Jack and Outlet Installation
| 9.2.3 | Two methods for mounting an RJ-45 jack

The telecommunications outlet in a horizontal cabling scheme is usually mounted on a wall. TIA/EIA-568-A specifies two types of wall mounts that you can use to position an RJ-45 jack onto a wall - the surface mount, and the flush mount.

| Web Links
| Cabling Glossary
| Cable Termination and Installation