B8ZS

  Binary 8-zero substitution. Line-code type, used on T1 and E1 circuits, in which a special code is substituted whenever 8 consecutive zeros are sent through the link. This code is then interpreted at the remote end of the connection. This technique guarantees ones density independent of the data stream. Sometimes called bipolar 8-zero substitution. Compare with AMI. See also ones density.

backbone

  The part of a network that acts as the primary path for traffic that is most often sourced from, and destined for, other networks.

backbone cabling

  Cabling that provides interconnections between wiring closets, wiring closets and the POP, and between buildings that are part of the same LAN. See vertical cabling.

back end

  Node or software program that provides services to a front end. See also client, front end, and server.

backoff

  The retransmission delay enforced when a collision occurs.

backplane

  Physical connection between an interface processor or card and the data buses and power distribution buses inside a Cisco chassis.

back pressure

  Propagation of network congestion information upstream through an internetwork.

backward explicit congestion notification

  See BECN.

backward learning

  Algorithmic process used for routing traffic that surmises information by assuming symmetrical network conditions. For example, if node A receives a packet from node B through intermediate node C, the backward-learning routing algorithm will assume that A can optimally reach B through C.

balanced configuration

  In HDLC, a point-to-point network configuration with two combined stations.

balanced, unbalanced

  See balun.

balun

  Balanced, unbalanced. Device used for matching impedance between a balanced and an unbalanced line, usually twisted-pair and coaxial cable.

bandwidth

  The difference between the highest and lowest frequencies available for network signals. The term is also used to describe the rated throughput capacity of a given network medium or protocol.

bandwidth allocation

  See bandwidth reservation.

bandwidth reservation

> Process of assigning bandwidth to users and applications served by a network. Involves ssigning priority to different flows of traffic based on how critical and delay-sensitive they are. This makes the best use of available bandwidth, and if the network becomes congested, lower-priority traffic can be dropped. Sometimes called bandwidth allocation. See also call priority.

banner motd

> Command used to configure a message of the day which is displayed at login and is useful for conveying messages that affect all network users, such as impending system shutdowns.

Banyan VINES

  See VINES.

BARRNet

  Bay Area Regional Research Network. Regional network serving the San Francisco Bay Area. The BARRNet backbone is composed of four University of California campuses (Berkeley, Davis, Santa Cruz, and San Francisco), Stanford University, Lawrence Livermore National Laboratory, and NASA Ames Research Center. BARRNET is now part of BBN Planet. See also BBN Planet.

baseband

  Characteristic of a network technology where only one carrier frequency is used. Ethernet is an example of a baseband network. Also called narrowband. Contrast with broadband.

bash

  Bourne-again shell. Interactive UNIX shell based on the traditional Bourne shell, but with increased functionality. The LynxOS bash shell is presented when you log in to a LightStream 2020 ATM switch as root (bash#) or fldsup (bash$). See also fldsup account and root account.

basic configuration

  The minimal configuration information entered when a new router, switch, or other configurable network device is installed on a network. The basic configuration for a LightStream 2020 ATM switch, for example, includes IP addresses, the date, and parameters for at least one trunk line. The basic configuration enables the device to receive a full configuration from the NMS.

basic encoding rules

> See BER.

Basic Rate Interface

  See BRI.

Basic Research and Human Resources

  See BRHR.

baud

  Unit of signaling speed equal to the number of discrete signal elements transmitted per second. Baud is synonymous with bits per second (bps), if each signal element represents exactly 1 bit.

Bay Area Regional Research Network

  See BARRNet.

BBN

  Bolt, Beranek, and Newman, Inc. High-technology company located in Massachusetts that developed and maintained the ARPANET (and later, the Internet) core gateway system. See also BBN Planet.

BBN Planet

  Subsidiary company of BBN that operates a nationwide Internet access network composed in part by the former regional networks BARRNET, NEARNET, and SURAnet. See also BARRNet, BBN, NEARNET, and SURAnet.

Bc

  Committed Burst. Negotiated tariff metric in Frame Relay internetworks. The maximum amount of data (in bits) that a Frame Relay internetwork is committed to accept and transmit at the CIR. See also Be and CIR.

B channel

  Bearer channel. In ISDN, a full-duplex, 64-kbps channel used to send user data. Compare to D channel, E channel, and H channel.

Be

  Excess Burst. Negotiated tariff metric in Frame Relay internetworks. The number of bits that a Frame Relay internetwork will attempt to transmit after Bc is accommodated. Be data is, in general, delivered with a lower probability than Bc data because Be data can be marked as DE by the network. See also Bc and DE.

beacon

  Frame from a Token Ring or FDDI device indicating a serious problem with the ring, such as a broken cable. A beacon frame contains the address of the station assumed to be down. See also failure domain.

bearer channel

  See B channel.

Because It's Time Network

  See BITNET.

BECN

  Backward explicit congestion notification. Bit set by a Frame Relay network in frames traveling in the opposite direction of frames encountering a congested path. DTE receiving frames with the BECN bit set can request that higher-level protocols take flow control action as appropriate. Compare with FECN.

Bell Communications Research

  See Bellcore.

Bellcore

  Bell Communications Research. Organization that performs research and development on behalf of the RBOCs.

Bellman-Ford routing algorithm

  See distance vector routing algorithm.

Bell operating company

  See BOC.

BER

  1. Bit error rate. The ratio of received bits that contain errors.
  2. Basic encoding rules. Rules for encoding data units described in the ISO ASN.1 standard. See also ASN.1.

Berkeley Standard Distribution

  See BSD.

BERT

  Bit error rate tester. Device that determines the BER on a given communications channel. See also BER (bit error rate).

best-effort delivery

  Describes a network system that does not use a sophisticated acknowledgment system to guarantee reliable delivery of information.

BGP

  Border Gateway Protocol. Interdomain routing protocol that replaces EGP. BGP exchanges reachability information with other BGP systems. It is defined by RFC 1163. See also BGP4 and EGP.

BGP4

  BGP Version 4. Version 4 of the predominant interdomain routing protocol used on the Internet. BGP4 supports CIDR and uses route aggregation mechanisms to reduce the size of routing tables. See also BGP and CIDR.

BIGA

  Bus Interface Gate Array. Technology that allows the Catalyst 5000 to receive and transmit frames from its packet-switching memory to its MAC local buffer memory without the intervention of the host processor.

big-endian

  Method of storing or transmitting data in which the most significant bit or byte is presented first. Compare with little-endian.

binary

  A numbering system characterized by ones and zeros (1 = on, 0 = off).

binary 8-zero substitution

  See B8ZS.

binary coded alternate mark inversion

  See AMI.

binary synchronous communication

  See BSC.

biphase coding

  Bipolar coding scheme originally developed for use in Ethernet. Clocking information is embedded into and recovered from the synchronous data stream without the need for separate clocking leads. The biphase signal contains no direct current energy.

bipolar

  Electrical characteristic denoting a circuit with both negative and positive polarity. Contrast with unipolar.

bipolar 8-zero substitution

  See B8ZS.

BISDN

  Broadband ISDN. ITU-T communication standards designed to handle high-bandwidth applications such as video. BISDN currently uses ATM technology over SONET-based transmission circuits to provide data rates from 155 to 622 Mbps and beyond. Contrast with N-ISDN. See also BRI, ISDN, and PRI.

bisync

  See BSC.

bit

  Binary digit used in the binary numbering system. Can be 0 or 1.

bit error rate

  See BER.

bit error rate tester

  See BERT.

BITNET

  "Because It's Time" Networking Services. Low-cost, low-speed academic network consisting primarily of IBM mainframes and 9600-bps leased lines. BITNET is now part of CREN. See also CREN.

BITNET III

  Dial-up service providing connectivity for members of CREN. See also CREN.

bit-oriented protocol

  Class of data link layer communication protocols that can transmit frames regardless of frame content. Compared with byte-oriented protocols, bit-oriented protocols provide full-duplex operation and are more efficient and reliable. Compare with byte-oriented protocol.

bit rate

  Speed at which bits are transmitted, usually expressed in bits per second (bps).

bits per second

  Abbreviated bps.

black hole

  Routing term for an area of the internetwork where packets enter, but do not emerge, due to adverse conditions or poor system configuration within a portion of the network.

blocking

  In a switching system, a condition in which no paths are available to complete a circuit. The term is also used to describe a situation in which one activity cannot begin until another has been completed.

block multiplexer channel

  IBM-style channel that implements the FIPS-60 channel, a U.S. channel standard. This channel is also referred to as OEMI channel and 370 block mux channel.

blower

  Internal cooling fan used in larger router and switch chassis such as the Cisco AGS+, the Cisco 7000, and the LightStream 2020.

BNC connector

  Short for British Naval Connector or Bayonet Nut Connector or Bayonet Neill Concelman, a type of connector used with coaxial cables such as the RG-58 A/U cable used with the 10BASE2 Ethernet system. The basic BNC connector is a male type mounted at each end of a cable. This connector has a center pin connected to the center cable conductor and a metal tube connected to the outer cable shield. A rotating ring outside the tube locks the cable to any female connector.

BNN

  Boundary network node. In SNA terminology, a subarea node that provides boundary function support for adjacent peripheral nodes. This support includes sequencing, pacing, and address translation. Also called boundary node.

BOC

  Bell operating company. See RBOC.

Bolt, Beranek, and Newman, Inc.

  See BBN.

BOOTP

  Protocol used by a network node to determine the IP address of its Ethernet interfaces, in order to affect network booting.

boot programmable read-only memory

  See boot PROM.

boot PROM

  Boot programmable read-only memory. Chip mounted on a printed circuit board used to provide executable boot instructions to a computer device.

border gateway

  Router that communicates with routers in other autonomous systems.

Border Gateway Protocol

  See BGP.

boundary function

  Capability of SNA subarea nodes to provide protocol support for attached peripheral nodes. Typically found in IBM 3745 devices.

boundary network node

  See BNN.

boundary node

  See BNN.

BPDU

  Bridge protocol data unit. Spanning-Tree Protocol hello packet that is sent out at configurable intervals to exchange information among bridges in the network. See also PDU.

bps

  Bits per second.

BRHR

  Basic Research and Human Resources. Component of the HPCC program designed to support research, training, and education in computer science, computer engineering, and computational science. See also HPCC.

BRI

  Basic Rate Interface. ISDN interface composed of two B channels and one D channel for circuit-switched communication of voice, video, and data. Compare with PRI. See also BISDN, ISDN, and N-ISDN.

bridge

  Device that connects and passes packets between two network segments that use the same communications protocol. Bridges operate at the data link layer (Layer 2) of the OSI reference model. In general, a bridge will filter, forward, or flood an incoming frame based on the MAC address of that frame. See also relay.

bridge forwarding

  Process that uses entries in a filtering database to determine whether frames with a given MAC destination address can be forwarded to a given port or ports. Described in the IEEE 802.1 standard. See also IEEE 802.1.

bridge group

  Cisco bridging feature that assigns network interfaces to a particular spanning-tree group. Bridge groups can be compatible with the IEEE 802.1 or the DEC specification.

bridge number

  Number that identifies each bridge in an SRB LAN. Parallel bridges must have different bridge numbers.

bridge protocol data unit

  See BPDU.

bridge static filtering

  Process in which a bridge maintains a filtering database consisting of static entries. Each static entry equates a MAC destination address with a port that can receive frames with this MAC destination address and a set of ports on which the frames can be transmitted. Defined in the IEEE 802.1 standard. See also IEEE 802.1.

broadband

  Transmission system that multiplexes multiple independent signals onto one cable. In telecommunications terminology, any channel having a bandwidth greater than a voice-grade channel (4 kHz). In LAN terminology, a coaxial cable on which analog signaling is used. Also called wideband. Contrast with baseband.

Broadband ISDN

  See BISDN.

broadcast

  Data packet that will be sent to all nodes on a network. Broadcasts are identified by a broadcast address. Compare with multicast and unicast. See also broadcast address.

broadcast address

  Special address reserved for sending a message to all stations. Generally, a broadcast address is a MAC destination address of all ones. Compare with multicast address and unicast address. See also broadcast.

broadcast and unknown server

  See BUS.

broadcast domain

  The set of all devices that will receive broadcast frames originating from any device within the set. Broadcast domains are typically bounded by routers because routers do not forward broadcast frames.

broadcast search

  Propagation of a search request to all network nodes if the location of a resource is unknown to the requester. See also directed search.

broadcast storm

  Undesirable network event in which many broadcasts are sent simultaneously across all network segments. A broadcast storm uses substantial network bandwidth and, typically, causes network time-outs.

browser

  See WWW browser.

BSC

  Binary synchronous communication. Character-oriented data link layer protocol for half-duplex applications. Often referred to simply as bisync.

BSD

  Berkeley Standard Distribution. Term used to describe any of a variety of UNIX-type operating systems based on the UC Berkeley BSD operating system.

BT

  Burst tolerance. Parameter defined by the ATM Forum for ATM traffic management. For VBR connections, BT determines the size of the maximum burst of contiguous cells that can be transmitted. See also VBR.

buffer

  Storage area used for handling data in transit. Buffers are used in internetworking to compensate for differences in processing speed between network devices. Bursts of data can be stored in buffers until they can be handled by slower processing devices. Sometimes referred to as a packet buffer.

burst tolerance

  See BT.

BUS

  Broadcast and unknown server. Multicast server used in ELANs that is used to flood traffic addressed to an unknown destination, and to forward multicast and broadcast traffic to the appropriate clients. See also ELAN.

bus

  1. Common physical signal path composed of wires or other media across which signals can be sent from one part of a computer to another. Sometimes called highway.
  2. See bus topology.

bus and tag channel

  IBM channel, developed in the 1960s, incorporating copper multiwire technology. Replaced by the ESCON channel. See also ESCON channel and parallel channel.

Bus Interface Gate Array

  See BIGA.

bus topology

  Linear LAN architecture in which transmissions from network stations propagate the length of the medium and are received by all other stations. Compare with ring topology, star topology, and tree topology.

bypass mode

  Operating mode on FDDI and Token Ring networks in which an interface has been removed from the ring.

bypass relay

  Allows a particular Token Ring interface to be shut down and thus effectively removed from the ring.

byte

  Term used to refer to a series of consecutive binary digits that are operated upon as a unit (for example, an 8-bit byte).

byte-oriented protocol

  Class of data-link communications protocols that use a specific character from the user character set to delimit frames. These protocols have largely been replaced by bit-oriented protocols. Compare with bit-oriented protocol.

byte reversal

  Process of storing numeric data with the least-significant byte first. Used for integers and addresses on devices with Intel microprocessors.