Backbone cabling design recommendations :: | 46/55

| Backbone cabling design recommendations

- The intrabuilding backbone subsystem should be designed with sufficient spare capacity to service additional outlet/connectors from the centralized cross-connect without the need to pull additional intrabuilding backbone cables.
- The intrabuilding backbone fiber count should be sized to deliver present and future applications to the maximum work area density within the area served by the telecommunications room.
- Generally, two fibers are required for each application delivered to a work area.

Backbone cabling design recommendations :: | 46/55