|  | 8.8 | Design Practice No. 1: Wiring Plan for Ethernet Star Topology LAN
| 8.8.7 | West building: second floor

During the preliminary survey, three potential locations for wiring closets were identified for the second floor of the west building. They are identified on the floor plan as U, V, and W.

1. Location U uses florescent lighting. The door opens out of the room and can be secured with a lock. The light switch is to the left of the door upon entering the room. The room has a dropped ceiling. Walls are covered with an asbestos material. There are four electrical outlets in the room.
2. Location V has interior water lines that pass through its dropped ceiling space and lead into adjacent men's and women's restrooms. The room uses incandescent lighting. The door opens out of the room and can be secured with a lock. The light switch is to the right of the door upon entering the room. The walls are covered with an asbestos material. There are four electrical outlets in the room.
3. Location W is near the front of the building. The room uses incandescent lighting. The door opens out of the room and can be secured with a lock. The light switch is to the right of the door upon entering the room. The walls are covered in a fire-retardant paint. There are two electrical outlets in the room.

| Web Links
| Cabling Glossary