|  | 10.7 | Creating a Subnet
| 10.7.6 | IP configuration on a network diagram

When you configure routers, you must connect each interface to a different network segment. Then each of these segments will become a separate subnet. You must select an address from each different subnet to assign to the interface of the router that connects to that subnet. Each segment of a network - the actual wires and links - must have different network/subnet numbers. The Figure shows what a network diagram might look like using a subnetted Class B network.

| Web Links

Introduction to the Internet Protocols